Notes for Sheet Metal Part Design Process:

* Find dimensions for press fit parts
* Press fit nuts and fixtures must be harder than material base
* http://www.pemnet.com/fastening\_products/pem-self-clinching-fastener\_new.html
* http://www.spyraflo.com/bearings/installation/press-fit/